SECTION 06 46 00 - WOOD TRIM

 GENERAL

 SUBMITTALS

 Action Submittals:

 Product Data: Manufacturer’s descriptive data and product attributes for trim.

 Samples: [Selection samples.] [Verification samples.]

 ADMINISTRATIVE REQUIREMENTS

 Pre-Installation Conference:

 Attendance: [Design Professional,] [Owner,] [Contractor,] [Construction Manager,] [Design/Builder,] installer, and related trades.

 Review: Critical dimensions, delivery and storage, staging and sequencing, and protection of completed work.

 QUALITY ASSURANCE

 Installer Qualifications: Firm specializing in work of this Section, with minimum [2] [\_\_] years’ experience.

 Mockups: [[8] [\_\_] feet long.] [\_\_\_\_.] Approved mockups [may] [may not] remain as part of the Work.

 WARRANTIES

 Primed SPF, Premium Primed and EvoTrim: Manufacturer’s 5-year limited warranty against primer peel and flake.

\*\*\*\* OR \*\*\*\*

 Premium Primed and EvoTrim: Manufacturer’s 20-year limited warranty against structural failure caused by glue joint delamination.

 \*\*\*\* OR \*\*\*\*

* + 1. EvoTrim: Manufacturer’s 40-year limited warranty against structural failure caused by fungal decay or termite attack.

 \*\*\*\* OR \*\*\*\*

* + 1. Thermally Modified Wood: Manufacturer’s 20-year limited warranty against rot and decay.

 PRODUCTS

 MANUFACTURERS

 Wood Trim: UFP Edge. [www.ufpedge.com](http://www.ufpedge.com/)

 Substitutions: [Refer to Division 01.] [Not permitted.]

 MATERIALS

 [Interior] [Exterior] Trim:

 Description: Wood thermally modified by controlled pyrolysis process.

 Species: Poplar (ForgeWood)

 Size: Nominally [1 x 4] [1 x 6] inches.

 Profile: Square Edge.

 Color: [Raw.] [Brass.] [Tungsten.] [Steel.] [Coal.] [To be selected from manufacturer’s full color range.]

 Surface texture: [Smooth – Raw only.] [Wire brushed – All other colors.]

 \*\*\*\* OR \*\*\*\*

 [Interior] [Exterior] Trim:

 Description: Wood thermally modified by controlled pyrolysis process.

 Species: Vertical grain Hemlock

 Size: Nominally [1 x 4] [1 x 6] [1 x 8] inches.

 Profile: Square Edge.

 Color: Natural.

 Surface texture: [Smooth.] [Wire brushed.]

\*\*\*\* OR \*\*\*\*

 [Interior] [Exterior] Trim:

 Source: Evotrim

 Description: Finger jointed and edge glued, then treated with TRU-CORE to resist termites and fungal decay.

 Preservative treatment: TRU-CORE.

 Species: Radiata Pine.

 Thickness: Nominally [1 inch.] [1-1/4 inches.] [2 inches.]

 Surface texture: [S1S2E.] [S4S.]

 Finish: Factory-applied exterior primer with mildewcide.

\*\*\*\* OR \*\*\*\*

 [Interior] [Exterior] Trim:

 Source: Premium Primed.

 Description: Finger jointed and edge glued, kiln dried.

 Species: Radiata Pine.

 Thickness: Nominally [1 inch.] [1-1/4 inches.] [2 inches.]

 Surface texture: [S1S2E.] [S4S.]

 Finish: Factory-applied exterior primer with mildewcide.

\*\*\*\* OR \*\*\*\*

 [Interior] [Exterior] Trim:

 Source: Primed SPF

 Description: Solid sawn, kiln dried.

 Species: Spruce/Pine/Fir.

 Thickness: Nominally [1 inch.] [1-1/4 inches.] [2 inches.]

 Surface texture: [S1S2E.] [S4S.]

 Finish: Factory-applied exterior primer with mildewcide.

 ACCESSORIES

 Fasteners: [Hot dip galvanized steel.] [Aluminum.] [Type [304] [316] stainless steel.] [Fluoropolymer coated steel.] [\_\_\_\_].

 FABRICATION

 Quality: AWI Architectural Woodwork Standards, [Premium] [Custom] Grade.

 EXECUTION

 INSTALLATION

 Install trim in accordance with manufacturer’s instructions and AWI Architectural Woodwork Standards.

 [Butt] [Miter] ends, corners, and intersections.

END OF SECTION