SECTION 06 46 29 – WOOD SOFFITS

 GENERAL

 SUBMITTALS

 Action Submittals:

 Product Data: Manufacturer’s descriptive data and product attributes for cladding.

 Samples: [Selection samples.] [Verification samples.]

 QUALITY ASSURANCE

 Installer Qualifications: Firm specializing in work of this Section with minimum [2] [\_\_] years’ experience.

 WARRANTIES

 Manufacturer’s 20-year limited warranty against rot and decay.

 PRODUCTS

 MANUFACTURERS

 Wood Soffits: UFP Edge. [www.ufpedge.com](http://www.ufpedge.com)

 Substitutions: [Refer to Division 01.] [Not permitted.]

 MATERIALS

 Wood Siding:

 Description: Wood thermally modified by controlled pyrolysis process.

 Species: Poplar (ForgeWood)

 Size: Nominally [1 x 6] [1 x 8] inches.

 Profile: Tongue and groove, nickel,gap reveal, end matched.

 Color: [Raw.] [Brass.] [Tungsten.] [Steel.] [Coal.] [To be selected from manufacturer’s full color range.]

 Surface texture: [Smooth – Raw only.] [Wire brushed – All other colors.]

\*\*\*\* OR \*\*\*\*

 Wood Soffits:

 Description: Wood thermally modified by controlled pyrolysis process.

 Species: Vertical grain Hemlock

 Size: Nominally [1 x 4] [1 x 6] inches.

 Profile: Tongue-and-groove, nickel gap, end matched.

 Color: Natural.

 Surface texture: [Smooth.] [Wire brushed.]

 ACCESSORIES

 Fasteners: Type [304] [316] stainless steel.

 EXECUTION

 INSTALLATION

 Install soffits in accordance with manufacturer's instructions.

END OF SECTION