SECTION 06 46 29 – WOOD SOFFITS

GENERAL

SUBMITTALS

Action Submittals:

Product Data: Manufacturer’s descriptive data and product attributes for cladding.

Samples: [Selection samples.] [Verification samples.]

QUALITY ASSURANCE

Installer Qualifications: Firm specializing in work of this Section with minimum [2] [\_\_] years’ experience.

WARRANTIES

Manufacturer’s 20-year limited warranty against rot and decay.

PRODUCTS

MANUFACTURERS

Wood Soffits: UFP Edge. [www.ufpedge.com](http://www.ufpedge.com)

Substitutions: [Refer to Division 01.] [Not permitted.]

MATERIALS

Wood Siding:

Description: Wood thermally modified by controlled pyrolysis process.

Species: Poplar (ForgeWood)

Size: Nominally [1 x 6] [1 x 8] inches.

Profile: Tongue and groove, nickel,gap reveal, end matched.

Color: [Raw.] [Brass.] [Tungsten.] [Steel.] [Coal.] [To be selected from manufacturer’s full color range.]

Surface texture: [Smooth – Raw only.] [Wire brushed – All other colors.]

\*\*\*\* OR \*\*\*\*

Wood Soffits:

Description: Wood thermally modified by controlled pyrolysis process.

Species: Vertical grain Hemlock

Size: Nominally [1 x 4] [1 x 6] inches.

Profile: Tongue-and-groove, nickel gap, end matched.

Color: Natural.

Surface texture: [Smooth.] [Wire brushed.]

ACCESSORIES

Fasteners: Type [304] [316] stainless steel.

EXECUTION

INSTALLATION

Install soffits in accordance with manufacturer's instructions.

END OF SECTION